# Author

Github: jnettlet


# Source Url:

99-asus-falchion.hwdb : [GITHUB](https://gist.github.com/jnettlet/afb20a048b8720f3b4eb8506d8b05643)

40-libinput.conf : [Ask Ubuntu](https://askubuntu.com/questions/1351203/how-do-i-stop-my-rog-falchion-wireless-keyboard-from-rebooting-ubuntu)

# Installation

## Common

```bash
cp ./99-asus-falchion.hwdb /etc/udev/hwdb.d/99-asus-falchion.hwdb
systemd-hwdb update

# or 

curl https://raw.githubusercontent.com/mrdev023/linux-conf/main/useful_scripts/falchion/install.sh -o - | bash
```

## X11

Append the following config to /usr/share/X11/xorg.conf.d/40-libinput.conf or use this and add it in startup script see `example_script.sh`

```bash
xinput disable XX # XX being the device id related to 'ASUSTeK ROG FALCHION System Control'
xinput disable "ASUSTeK ROG FALCHION System Control"
xinput disable "ASUSTeK ROG FALCHION Consumer Control"
xinput disable "ASUSTeK ROG GLADIUS III WIRELESS System Control"
xinput disable "ASUSTeK ROG GLADIUS III WIRELESS Consumer Control"
```